# Nmap 7.93 scan initiated Tue Apr  2 16:28:32 2024 as: nmap -A -p 25,465 --script vuln -oN /opt/i_nmap_stare_smtp_vuln.txt smtp.vsb.cz
Nmap scan report for smtp.vsb.cz (158.196.149.155)
Host is up (0.00033s latency).
Other addresses for smtp.vsb.cz (not scanned): 2001:718:1001:149::155

PORT    STATE SERVICE  VERSION
25/tcp  open  smtp     Postfix smtpd
| smtp-vuln-cve2010-4344: 
|_  The SMTP server is not Exim: NOT VULNERABLE
465/tcp open  ssl/smtp Postfix smtpd
| smtp-vuln-cve2010-4344: 
|_  The SMTP server is not Exim: NOT VULNERABLE
| ssl-dh-params: 
|   VULNERABLE:
|   Anonymous Diffie-Hellman Key Exchange MitM Vulnerability
|     State: VULNERABLE
|       Transport Layer Security (TLS) services that use anonymous
|       Diffie-Hellman key exchange only provide protection against passive
|       eavesdropping, and are vulnerable to active man-in-the-middle attacks
|       which could completely compromise the confidentiality and integrity
|       of any data exchanged over the resulting session.
|     Check results:
|       ANONYMOUS DH GROUP 1
|             Cipher Suite: TLS_DH_anon_WITH_CAMELLIA_256_CBC_SHA256
|             Modulus Type: Safe prime
|             Modulus Source: Unknown/Custom-generated
|             Modulus Length: 2048
|             Generator Length: 8
|             Public Key Length: 2048
|     References:
|_      https://www.ietf.org/rfc/rfc2246.txt
Warning: OSScan results may be unreliable because we could not find at least 1 open and 1 closed port
Device type: general purpose|specialized|media device|WAP
Running (JUST GUESSING): Linux 4.X|5.X|2.6.X|3.X (93%), Crestron 2-Series (90%), Motorola embedded (88%), Lorex embedded (88%), Sony embedded (88%), Asus embedded (87%)
OS CPE: cpe:/o:linux:linux_kernel:4 cpe:/o:linux:linux_kernel:5 cpe:/o:linux:linux_kernel:2.6.32 cpe:/o:crestron:2_series cpe:/h:lorex:nv408 cpe:/h:asus:rt-n56u cpe:/o:linux:linux_kernel:3.4
Aggressive OS guesses: Linux 4.15 - 5.6 (93%), Linux 5.0 - 5.4 (93%), Linux 5.3 - 5.4 (93%), Linux 2.6.32 (92%), Linux 5.0 (92%), Linux 5.0 - 5.3 (92%), Linux 5.4 (90%), Crestron XPanel control system (90%), Motorola KreaTV (Linux 2.6.32) (88%), Lorex NV408 video recorder (88%)
No exact OS matches for host (test conditions non-ideal).
Network Distance: 2 hops
Service Info: Host:  smtp.vsb.cz

TRACEROUTE (using port 465/tcp)
HOP RTT     ADDRESS
1   0.26 ms 158.196.94.2
2   0.35 ms smtp.vsb.cz (158.196.149.155)

OS and Service detection performed. Please report any incorrect results at https://nmap.org/submit/ .
# Nmap done at Tue Apr  2 16:29:00 2024 -- 1 IP address (1 host up) scanned in 28.29 seconds
